SNR Map (from ABCD QA)

|  |  |
| --- | --- |
| Premier 48-ch  | MR750 32-ch Nova |
|  |  |
| meanBkgnd = 118.2885meanSignal = 956.7254signal/noise(mean\_background) = 8.0881 | meanBkgnd = 26.4690meanSignal = 259.3045signal/noise(mean\_background) = 9.7965 |
|  |